12-8 Main Technological Economy Indicators of Railway Transportation
Item | 2000 | 2003
Average Daily Ton-kilometers of Freight Locomotives (10 000 ton-km) | 107.1 | 96.7
Diesel Locomotives | 107.1 | 96.7
Average Total Tonnage of Freight Locomotives (ton) | 2327 | 2342
Diesel Locomotives | 2327 | 2342
Daily Distance per Freight Locomotive (km) | 610 | 573
Daily Distance per Passenger Locomotive (km) | 627 | 720
Oil Consumption of Diesel Locomotives (kg/10 000 ton-km) | 27.6 | 30.5
Punctuality Rate of Freight Trains at Departure (%) | 99.4 | 98.5
Punctuality Rate of Freight Trains in Running (%) | 97.2 | 92
Punctuality Rate of Passenger Trains at Departure (%) | 99.7 | 97.2
Punctuality Rate of Passenger Trains in Running (%) | 99.5 | 97.2
Technical Speed of Passenger Trains (km/hr) | 62.3 | 70.7
Travelling Speed of Passenger Trains (km/hr) | 57.7 | 62.1
Density of Passenger Transport (10 000 passenger-km/km) | 323.6 | 366.9
Technical Speed of Freight Trains (km/hr) | 46.9 | 48.2
Running Speed of Freight Trains (km/hr) | 43.6 | 36.2
Density of Freight Transport (10 000 ton-km/km) | 1179.3 | 1577
Turning Around Time of Freight Cars (day) | 4.65 | 5.23
Handling Time of Freight (hour) | 38.9 | 25.3
Transfer Waiting Time per Car (hour) | 3.6 | 4.9
Static Load of Freight Cars (Standard Gauge) (ton) | 52.8 | 55.3